**SPP00350 (01-01-21) *(This section may require SPP02320 if using MSE***  ***Retaining Walls)***

### Section 00350 - Geosynthetic Installation

Comply with section 00350 of the Standard Construction Specifications modified as follows:

***(Place an "X" next to the appropriate geotextile types and under the appropriate level. Delete what does not apply. Delete the level not used. Obtain Geogrid information from the designer.)***

**00350.10 Materials** - Add the following to the end of this subsection:

Provide manufacturer's certifications complying with section 02320.10(c) for the following geosynthetic(s):

 **Certification**

**Geotextile Level A Level B**

Drainage, Type 1 \_\_\_\_\_\_\_ \_\_\_\_\_

Drainage, Type 2 \_\_\_\_\_ \_\_\_\_\_\_

Riprap, Type 1

Riprap, Type 2

Subgrade

Embankment

Pavement Overlay

**Geogrid**