***SPP00405 (01-01-21) (May require USP01091 Stream Restoration)***

***(Follow all instructions.  If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications.  Delete specifications that do not apply to the project.  Remove all instructions before preparing the final document.)***

### **Section 00405 - Trench Excavation, Bedding and Backfill**

Comply with section 00405 of the Standard Construction Specifications modified as follows:

***(Consider the use of the following subsections in large projects to limit the sprawl of Contractor’s work in numerous sites. This is intended to mandate the Contractor to finish the work in its entirety in four blocks at a time.)***

Add the following subsections:

**00405.41(a) Within Paved Areas to Be Preserved:**

**(3) Work Limits** - Contractor’s work must be completed within a designated work limit prior to initiating work within another designated work limit area. The typical work limits delineation is four (4) blocks. Owner’s Representative can approve alteration to the work limits.

**(4) Unfinished Work** - Work within any designated work limit will be considered unfinished until the work limit area can safely be reopened for public access and all the following tasks have been completed:

1. Surface Removal
2. Excavation
3. Mainline and service lateral construction
4. Backfilling with compaction
5. Pavement base construction
6. Final surface restoration
7. Sidewalk and driveway construction
8. Landscaping
9. Property restoration
10. Pipe acceptance testing
11. Site cleanup

***(Designer Note: Needed when the Stream Restoration Unique Specification 01091 used.)***

**00405.46(f) Restoration of Streambeds** – Replace the first sentence with the following:

Comply with Sections 00280, 00290.30(a), and 01091. Upon completion of the work: