**SPP00730 (01-01-21) (This Section requires SPP00640)**

***(Follow all instructions. If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications. Delete specifications that do not apply to the project. Remove all instructions before preparing the final document.)***

### Section 00730 – Emulsified Asphalt Tack Coat

Comply with section 00730 of the Standard Construction Specifications modified as follows:

***(Use when paving streets with multiple lifts of asphalt pavement. Obtain quantities from the designer. Typical application rate is 0.15 gallons/square yard with asphalt tack weighing 8 pounds/gallon.)***

**00730.80 Asphalt** – Add the following sentence.

Approximately \_\_\_\_\_ tons of asphalt in tack coat will be required on this Project.