**SPP00748 (01-01-21) *(This section requires SP02320 when***

 ***subgrade geotextile is used.)***

***(Follow all instructions. If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications. Delete specifications that do not apply to the project. Remove all instructions before preparing the final document.)***

***(Use this specification when CLSM will be used as backfill for narrow asphalt repairs ( < 1 ft. wide ) such as along curb extensions or replaced curb/driveway installations.)***

### Section 00748 - Asphalt Concrete Pavement Repair

Comply with section 00748 of the Standard Construction Specifications modified as follows:

**00748.90 Payment** - Replace the first sentence with the following:

No separate or additional payment will be made for excavation, geotextile, stone embankment, aggregate, controlled low strength material, or water.