**SPP850 (01-01-21)**

***(When this Section is used on a project and when it has a completion date of September 15 or later, contact the Scheduler to determine if a separate completion date for striping is required. If a separate completion date is required, include an interim completion date in 00180.50(h).)***

***(Follow all instructions. If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications. Delete specifications that do not apply to the project. Remove all instructions before preparing the final document.)***

### Section 00850 - Common Provisions for Pavement Markings

Comply with Section 00850 of the Standard Construction Specifications modified as follows:

***(Use the following when curb paint is included in project.)***

**00850.10 Materials** - Add the following bullet to the end of the bullet list:

* Curb Markings – Paint

***(Use the following when the project has either partial or no striping plans.)***

**00850.40 Plans** ‑ Add the following first sentence to this subsection:

For projects with partial striping plans or projects without striping plans, document all existing striping that is not shown in the supplemental drawings. Submit documentation to the Owner at least seven (7) calendar days before the loss of existing pavement markings.

***(Use the following subsection 00850.43 when traffic separators are required.)***

**00850.43 Striping Layout** - Replace the title of this subsection with the following:

**00850.43 Striping & Traffic Separator Layout**

***(Use the following subsection 00850.43 on all projects with striping.*** ***Delete language in red parentheses that does not apply, delete parentheses, and change red text to black.)***

**00850.43 Striping** ***(*and Traffic Separator*)* Layout** – Insert the following at the beginning of this subsection:

***(Use one of the following two paragraphs as indicated below. Delete the ones that do not apply.*** ***Delete language in red parentheses that does not apply, delete parentheses, and change red text to black.)***

***(Option 1 – Use this paragraph on all Federally Funded projects and use this paragraph when the striping is simple enough that you expect the Contractor to be able to perform striping layout.)***

The Owner will not provide construction staking of control points. Striping layout shall be the responsibility of the Contractor. Do not proceed with striping installation until the layout is approved by the Owner.

***(***For traffic separator layout, place control points centered at each end of a consecutive separator run.  Do not install separators until the layout is approved by the traffic engineer.***)***

The striping ***(***and traffic separator***)*** layout must be approved a minimum of two (2) calendar days prior to permanent striping operations. A request to approve the striping ***(***and traffic separator***)*** layout must be submitted to the Owner’s Representative a minimum of three (3) working days prior to the striping ***(***and traffic separator***)*** layout.

***(Option 2 – Use this paragraph when the striping is complex or extensive enough that survey construction staking is required, or you intend to provide construction staking yourself. Delete language in red parentheses that does not apply, delete parentheses, and change red text to black.)***

The Owner is responsible for construction staking of control points for striping ***(***and traffic separator***)*** layout per section 00150.15. The Contractor provides support, which includes, but is not limited to TCM, personnel, equipment, and material. Striping layout shall be the responsibility of the Contractor. Using these control points, layout a continuous narrow guideline for each line, along one edge of, or uniformly offset from the intended permanent line location. Do not proceed with striping ***(***or traffic separator***)*** installation until the layout is approved by the traffic engineer.

The striping ***(***and traffic separator***)*** layout must be approved a minimum of two (2) calendar days prior to permanent striping operations. A request to approve the striping ***(***and traffic separator***)*** layout must be submitted to the Owner’s Representative a minimum of three (3) working days prior to the striping ***(***and traffic separator***)*** layout.

***(Use the following on all projects.)***

**00850.44 Installation** - Replace the bullet that begins with “Place material according to…” with the following bullet:

* Place material according to the manufacturer’s installation instructions.

***(Use the following on all projects when 00868 is included in the special provisions.)***

**00850.47(c) Retroreflectivity** - Replace the sentence that begins "Except for paint applications…" with the following sentence:

Except for paint and colored lane marking applications, evaluate longitudinal and transverse marking retroreflectivity according to ODOT TM 777.