***SPP00930 (01-01-21)***

***(Follow all instructions. If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications. Delete specifications that do not apply to the project. Remove all instructions before preparing the final document.)***

**Section 00930 – Metal Sign Supports**

Comply with Section 00930 of the Standard Specifications modified as follows:

(Use the following subsection .10 when PSST sign supports are required.)

**00930.10 Materials** - Replace the paragraph that begins “Furnish structural steel materials…” with the following paragraph:

Furnish perforated steel square tube slip base sign supports and perforated steel square tube anchor sign supports from the CPL. Furnish other structural steel materials meeting the applicable portions of section 02530, with weights and sizes as shown or specified.

(Use the following on all projects)

**00930.40(e)(1) General** – Add the following sentence to the end of the paragraph:

The installation will be rejected if the geometry does not satisfy the requirements of section 02560.05.

***(Use the following subsection .80 to list the estimated quantities of steel. Delete rows inapplicable to the project. For 2-inch schedule 40 pipe sign posts, use 3.65 lbs/ft)***

**00930.80 Measurement** - Add the following to the end of this subsection:

The estimated quantities of structural steel are as follows:

 **Item** **Estimated Quantity**

 **(Pound)**

**Minor Sign Supports**

Triangular Base Breakaway Sign Supports \_\_

Perforated Steel Square Tube Slip Base Sign Supports \_\_

Pipe Sign Supports \_\_

Perforated Steel Square Tube Anchor Sign Supports \_\_