**SPP940 (01-01-21) *(This Section requires SPP2910.)***

***(Follow all instructions. If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications. Delete specifications that do not apply to the project. Remove all instructions before preparing the final document.)***

**Section 00940 - Signs**

Comply with section 00940 of the Standard Construction Specifications modified as follows:

***(Add the following on all projects.)***

Add the following subsection:

**00940.1 Sign Coatings** - Furnish all signs on the Project with a shop‑applied anti‑graffiti coating on both the background and legend sheeting according to 02910.70, regardless of substrate material.

***(Add the following on all projects.)***

**00940.40 General** - Add the following sentence to the end of the paragraph that begins “Fabricate all components…”:

For signs that require anti‑graffiti coating, fabricate all components of each individual sign with sheeting and anti-graffiti coating from the same supplier to ensure that all components are compatible and are warrantable by the manufacturer.

***(Add the following if required by the traffic engineer)***

**00940.46 Inspection** - Add the following to the end of this subsection:

The sign staking shall be the responsibility of the Contractor. Do not proceed with installation of new signs in new locations until the staked sign locations are approved by the traffic engineer.

(Use the following lead-in paragraph and subsection .48 when backs of aluminum substrate signs are coated. Obtain color number from Designer.)

Add the following subsection:

**00940.48 Coating** - Prepare and powder coat the backs of aluminum substrate signs according to the applicable portions of Section 00593 or prepare and coat according to the applicable portions of Section 00594.

Provide SAE AMS-STD-595 Color Number \_\_\_\_\_\_\_\_.