**USP910 (05-17-21)**

***(Follow all instructions. If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications. Delete specifications that do not apply to the project. Remove all instructions before preparing the final document.)***

## **Section 00910 - Wood Sign Posts**

Section 00910, which is not a standard specification, is included in this project by special provision.

**Description**

00910.00 **Scope** - This work consists of furnishing and installing preservative treated wood sign posts at the locations shown or as directed.

**Materials**

00910.10 **Materials** - Furnish Douglas fir wood posts meeting the following requirements:

Posts 02110.40

Preservative Treatment of Posts 02190

**Construction**

00910.40 **Post Holes** - Excavate post holes to the lines and grades established and to the depth shown or to a depth necessary to achieve the required mounting height, whichever is greater. If necessary, obtain the required depth by blasting. Do not set the post until the location, lines and grades of the holes have been approved. Align the post to a vertical position in the hole and backfill the hole. Backfill with selected general backfill meeting the requirements of 00330.13. Place in layers not greater than 6 inches. Solidly ram and tamp the layers into the excavated area around the post. Dampen during placement if too dry to compact properly. On completion of the work, replace and finish the surface around the post to match the surrounding surface.

**Measurement**

00910.80 **Measurement** - The quantities of wood sign posts will be measured on the volume basis, in units of foot board measure (FBM). Post volume will be determined by multiplying the nominal post size by the commercially available length shown on the standard drawings. For calculation purposes, post length will be determined by rounding the installed length to the nearest higher commercial length.

The estimated wood post lengths will be indicated on the plans. Final lengths of wood posts will be determined or verified by the Owner’s Representative prior to fabrication.

**Payment**

00910.90 **Payment** - The accepted quantities of wood sign posts will be paid for at the Contract unit price, per foot board measure (FBM), for the item "Wood Sign Posts".

Payment will be payment in full for furnishing and placing all materials, and for furnishing all equipment, labor, and incidentals necessary to complete the work as specified.

No separate or additional payment will be made for route marker frames, wind bracing, or special sign brackets.