**SPP227 (11-13-2020)**

***(Follow all instructions. If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications. Delete specifications that do not apply to the project. Remove all instructions before preparing the final document.)***

## Section 00227 - Temporary Traffic Signals and Illumination

(Use the following lead-in paragraph when any of the following subsections are included in the project.)

Comply with Section 00227 of the Standard Specifications modified as follows:

(Use the following subsection .40 only when vehicular traffic will be passing beneath falsework.)

**00227.40 Temporary Illumination** - Add the following paragraph to the end of this subsection:

Install 25‑watt, steady-burning, amber lights on 36‑inch spacing around the perimeter of the falsework as shown, facing oncoming traffic.

(Use the following subsection .90 only when vehicular traffic will be passing beneath falsework.)

**00227.90 Payment** – Add the following paragraph to the end of this subsection:

Item (a) includes all materials called for by the plans and specifications, and providing electrical power and furnishing, placing, maintaining, adjusting, and removing temporary falsework illumination.