**SPP00398 (01-01-21) *(This section may require S.)***

***(Follow all instructions.  If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications. Delete specifications that do not apply to the project.  Remove all instructions before preparing the final document.)***

### Section 00398 - Rock Slope Stabilization and Reinforcement

Comply with section 00398 of the Standard Construction Specifications modified as follows:

**00398.03(a) Rock Reinforcing Bolt and Rock Reinforcing Dowel Submittals ‑** Replace the paragraph that begins "Submit a detailed work plan …" with the following paragraph:

Submit a detailed work plan according to 00150.37 to the Owner’s Representative at least 10 (ten) Calendar Days prior to the preconstruction conference. Include the following:

**00398.03(b)(2) Work Plan** ‑ Replace the paragraph that begins "Submit a detailed work plan …" with the following paragraph:

Submit a detailed work plan to the Owner’s Representative at least 10 (ten) Calendar Days prior to the preconstruction conference. Include the following:

**00398.03(c) Anchored High Tensile Strength Wire Mesh Slope Protection Submittals** ‑ Replace the paragraph that begins "Submit a detailed work plan …" with the following paragraph:

Submit a detailed work plan according to 00150.37 to the Owner’s Representative for approval, at least 10 (ten) Calendar Days before the preconstruction conference. Include the following:

**00398.32 Rock Reinforcing Bolt and Rock Reinforcing Dowel Installation Personnel** ‑ Replace the paragraph that begins "Furnish personnel skilled in the …" with the following paragraph:

Furnish personnel skilled in the installation of Rock reinforcing bolts and Rock reinforcing dowels. Experience shall be relevant to anticipated Rock conditions and size of Rock reinforcing bolts and Rock reinforcing dowels being installed. The on-site supervisor and drill operator shall have no less than 2 (two) years of demonstrated experience in Rock reinforcing bolt and Rock reinforcing dowel installation. Submit documentation of experience to the Owner’s Representative at least 10 (ten) Calendar Days prior to the preconstruction conference. Include names and current phone numbers of references, project names and locations, and the year of project completion.