**SPP00406 (04-13-22 SSC)**

### Section 00406 – Tunneling, Boring and Jacking

Comply with section 00406 of the 2020 Standard Construction Specifications modified as follows:

**(*Use only on BES Projects as approved by the Construction Manager and Senior Inspector to be appropriate)***

**00406.92 Separate Unit Basis** – Replace the paragraph beginning with “Item (b)..” with the following:

For item (b), the nominal pipe size will be inserted in the blank. Item (b) includes all excavation, shafts, portals, jacking pits, pipe, conduits, pipe bedding, backfill, lubricant, grouting pipe, casing, rock removal, and all approved appurtenances.