**SPP00749 (01-01-21) (This section may require SPP00850 00867.42)**

### Section 00749 - Miscellaneous Asphalt Concrete Structures

Comply with section 00749 of the Standard Construction Specifications modified as follows:

***(Use the following subsection .00, .48 and .92 when constructing asphalt speed bumps.)***

**00749.00 Scope** – Add the word “speed bumps” to the end of the first sentence.

***(Use the following lead-in paragraph and subsections .14, and .47 on projects with asphalt islands.)***

Add the following subsections:

**00749.14 Concrete** - Furnish commercial grade concrete meeting the requirements of section 00440, section 00744.

**00749.47 Concrete** - Construct concrete curbs according to the applicable provisions of section 00759.

***(Use the following subsections .48 & .92 when constructing asphalt speed bumps. Requires the use of 00850.45)***

**00749.48 Speed Bumps** – Replace speed bump in its entirety as shown in the Contract Documents or as directed by the Owner’s Representative. Partial speed bump replacement is not allowed.

**00749.92 Method “B” – Complete in Place Basis** - Add the following:

 **Pay Item Unit of Measurement**

 (g) Asphalt Speed Bumps Each or Square Foot

Item (g) includes placing of materials, including asphalt concrete and asphalt tack coat, furnishing equipment, labor and incidentals necessary to complete asphalt speed bump in place as specified in the Contract Documents.

When included in the Contract schedule of items, the transverse pavement markings inlaid into the speed bumps will be paid for according to section 00867.

No additional payment will be made for removal of existing speed bumps.

***(Use the following subsection .92 on projects with asphalt islands.)***

**00749.92 Method "B" Complete in Place Basis** - Add the following sentence after the paragraph that begins "Item (c) includes…":

Item (c) This item also includes concrete curbs constructed with the asphalt islands.