**SPP00756 (09-01-20) *(This section requires SP02050, SP02440, and SP02530.)***

***(Follow all instructions. If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications. Delete specifications that do not apply to the project. Remove all instructions before preparing the final document.)***

### Section 00756 - Plain Concrete Pavement

Comply with section 00756 of the Standard Construction Specifications modified as follows:

***(Use the following lead-in paragraph and subsection .55 when the project length is less than 0.6 mile) and graphic profile testing is required. Check with Pavement Section when to use.)***

**00756.55 Surface Tolerance, Testing, and Correction** - Replace the first sentence with the following:

Perform graphic profile testing on this project.