SPP00868 (01-01-21) *(This Section requires SPP00850.)*

***(Follow all instructions. If there are no instructions above a subsection, paragraph, sentence or bullet, then include them in the project but make necessary modifications to only include project specific specifications. Delete specifications that do not apply to the project. Remove all instructions before preparing the final document.)***

***(Use the following when red transit markings are included in project.)***

## Section 00868 - Colored Lane Markings

Comply with Section 00868 of the Standard Construction Specifications modified as follows:

**00868.75(b) Failure** –Replace the first bullet with the following:

* Insufficient Color Stability:
* Green markings fail to meet the requirements of the Federal Highway Administration Interim Approval for Optional Use of Green Colored Pavement for Bike Lanes (IA-14) tested according to ASTM D6628.
* Red markings fail to meet the requirements of the Federal Highway Administration *Interim Approval for the Optional Use of Red‑Colored Pavement for Transit Lanes (IA‑22)* tested according to ASTM D6628.

***(When only one pay item is required, remove the “s” from “items” and delete the pay item that does not apply.)***

**00868.90 Payment** –Add the following pay itemsto the pay item list:

(c) Red Transit Lane, Preformed Thermoplastic Film……….Square Foot

(d) Red Transit Lane, Methyl Methacrylate…………………..Square Foot